The following is a new submission for order number FXA10291FA31

This folder contains 6 files which correspond to the following: 

Top Copper      laser_driver.TOP
Top Silk        laser_driver.TS
Top Resist      laser_driver.TR
Bottom Resist   laser_driver.BR
Bottom Copper   laser_driver.BOT
Drill           laser_driver.DRL
information file laser_driver.INF

My software is set to place the board outline in all files.

I did not supply a Top Mask file or Bottom Mask file. This is because my software does not produce mask file information.

I have supplied a Top and Bottom resist file. I _do_ want solder resist for the top and bottom layers. (Contrary to a previous message).

I did not supply a Bottom Silk file. This is because I do not want the bottom of the pcb to be silk screened. 

As per your specifications, all spacing is greater than 7 mils.  The previous file had a number of spacing problems which I have corrected, thank you for notifying me of the problems.

The attached file is a compressed zip file, it does not have a .zip extension because my mailer wont allow transfer of files with those extensions.




    Thank you,

            Owen White

 

 

