LABCENTER PROTEUS TOOL INFORMATION FILE
=======================================

In case of difficulty, please email support@labcenter.co.uk

Tool set up for C:\Program Files\Proteus\spam_driver\spam_driver.LYT

File List
---------
Top Copper      c:\documents and settings\owhite\desktop\laser_driver\laser_driver.TOP
Bottom Copper   c:\documents and settings\owhite\desktop\laser_driver\laser_driver.BOT
Top Silk        c:\documents and settings\owhite\desktop\laser_driver\laser_driver.TS
Top Resist      c:\documents and settings\owhite\desktop\laser_driver\laser_driver.TR
Bottom Resist   c:\documents and settings\owhite\desktop\laser_driver\laser_driver.BR
Drill           c:\documents and settings\owhite\desktop\laser_driver\laser_driver.DRL

Photoplotter Setup
------------------
Format: RS274X, ASCII, 2.4, imperial, absolute, eob=*, LZO
Notes:  D=Diam, S=Side, W=Width, H=Height

D10	CIRCLE	D=12th                                      DRAW
D11	CIRCLE	D=50th                                      FLASH
D12	SQUARE	S=80th                                      FLASH
D13	CIRCLE	D=80th                                      FLASH
D14	CIRCLE	D=70th                                      FLASH
D15	CIRCLE	D=250th                                     FLASH
D16	SQUARE	S=70th                                      FLASH
D17	SQUARE	S=50th                                      FLASH
D18	CIRCLE	D=60th                                      FLASH
D19	CIRCLE	D=200th                                     FLASH
D70	CIRCLE	D=90th                                      FLASH
D71	CIRCLE	D=150th                                     FLASH
D20	CIRCLE	D=8th                                       DRAW
D21	SQUARE	S=100th                                     FLASH
D22	CIRCLE	D=100th                                     FLASH
D23	CIRCLE	D=290th                                     FLASH
D24	SQUARE	S=90th                                      FLASH
D25	CIRCLE	D=240th                                     FLASH
D26	CIRCLE	D=410th                                     FLASH
D27	CIRCLE	D=110th                                     FLASH
D28	CIRCLE	D=190th                                     FLASH

NC Drill Setup
--------------
Format: ASCII, 2.4, imperial, absolute, eob=<CR><LF>, no zero suppression.
Notes:  Tool sizes are diameters. Layer sets are in brackets - 0=TOP, 15=BOTTOM, 1-14=INNER.

T01	20th (0-15)
T02	40th (0-15)
T03	30th (0-15)
T04	118.1th (0-15)
T05	80th (0-15)
T06	157.4th (0-15)
T07	25th (0-15)
T08	50th (0-15)
T09	130th (0-15)

